Combine the use of encoders and gyroscopes to do the following
- Drive forward 60 inches
- Rotate to 45 degrees (assume a left turn is negative rotation, right turn is positive rotation)
- Drive forward 20 inches
- Rotate to -90 degrees